

**AVAILABLE MODEL**

**Accessary of Magnetic Lock**

**DS-K4H258-LZ**

DS-K4H258-LZ LZ-Bracket of Magnetic Lock

**MAIN FEATURES**

|  |  |
| --- | --- |
| * Adopts aldural material
* Hard anodizing electroplating operated
* L-bracket is used for fixing the lock body;

Z-bracket is used for fixing the armature plate* Suitable for wooden door, and metal door
 |  |

**SPECIFICATIONS**

| **Model** | **DS-K4H258-LZ** |
| --- | --- |
| **L-bracket Dimension (L×W×H)**  | 238×30×47mm (9.4×1.2×1.9") |
| **Z-bracket Dimension (L×W×H)** | 185×44×100mm (7.3×1.7×3.9") |
| **Suitable Door** | Wooden Door, and Metal Door |
| **Shell Performance** | Hard Anodizing Electroplated |
| **Weight** | 0.77kg |

**INSTALLATION**



