

**AVAILABLE MODEL**

**Accessary of Magnetic Lock**

**DS-K4H258-U**

DS-K4H258-U U-Bracket of Magnetic Lock

**MAIN FEATURES**

|  |  |
| --- | --- |
| * Adopts aldural material
* Used for fixing the armature plate
* Hard anodizing electroplating operated
* Suitable for lower edge frameless glass door
 |  |

**SPECIFICATIONS**

| **Model** | **DS-K4H258-U** |
| --- | --- |
| **Dimension (L×W×H)**  | 185×28×45mm (7.3×1.1×1.8") |
| **Suitable Door** | Lower Edge Frameless Glass Door |
| **Shell Performance** | Hard Anodizing Electroplated |
| **Weight** | 0.4kg |

**INSTALLATION**

|  |  |
| --- | --- |
|  |  |